CANON SOFTWARE LICENSE AGREEMENT

IMPORTANT!

This is a legal agreement ("Agreement") between you and Canon Inc. ("Canon") 
and governing your use of Canon's software programs including the related 
manuals or any printed material thereof (the "Software") for certain Canon's 
copying machines, printers and multifunctional peripherals (the "Products").

READ CAREFULLY AND UNDERSTAND ALL OF THE RIGHTS AND
 RESTRICTIONS DESCRIBED IN THIS AGREEMENT BEFORE USING THE 
SOFTWARE.  BY THE ACTION TO INDICATE YOUR ACCEPTANCE OR 
USING THE SOFTWARE, YOU AGREE TO BE BOUND BY THE TERMS AND 
CONDITIONS OF THIS AGREEMENT.  IF YOU DO NOT AGREE TO THE 
FOLLOWING TERMS AND CONDITIONS OF THIS AGREEMENT, DO NOT 
USE THE SOFTWARE.  NO REFUND WILL BE MADE BECAUSE THE 
SOFTWARE WAS PROVIDED TO YOU AT NO CHARGE.


1.  GRANT OF LICENSE
Canon grants you a personal, limited and non-exclusive license to use ("use" 
as used herein shall include storing, loading, installing, accessing, executing
or displaying) the Software solely for the use with Products only on computers 
directly or via network connected to the Products (the "Designated Computer"). 
You may allow other users of other computers connected to your Designated 
Computer to use the Software, provided that you must assure that all such users
shall abide by the terms of this Agreement and shall be subject to restrictions
and obligations borne by you hereunder.

You may make one copy of the Software solely for a back-up purpose.

2.  RESTRICTIONS
You shall not use the Software except as expressly granted or permitted herein,
and shall not assign, sublicense, sell, rent, lease, loan, convey or transfer 
to any third party the Software.  You shall not alter, translate or convert to 
another programming language, modify, disassemble, decompile or otherwise 
reverse engineer the Software and you shall not have any third party to do so.

3.  COPYRIGHT NOTICE
You shall not modify, remove or delete any copyright notice of Canon or its 
licensors contained in the Software, including any copy thereof.

4.  OWNERSHIP
Canon and its licensors retain in all respects the title, ownership and 
intellectual property rights in and to the Software.  Except as expressly 
provided herein, no license or right, express or implied, is hereby conveyed or
granted by Canon to you for any intellectual property of Canon and its 
licensors.

5.  EXPORT RESTRICTION
You agree to comply with all export laws and restrictions and regulations of 
the country involved, and not to export or re-export, directly or indirectly, 
the Software in violation of any such laws, restrictions and regulations, or 
without all necessary approvals.

6.  NO SUPPORT
NEITHER CANON, CANON'S SUBSIDIARIES OR AFFILIATES, THEIR 
DISTRIBUTORS, OR DEALERS NOR CANON'S LICENSORS ARE 
RESPONSIBLE FOR MAINTAINING OR HELPING YOU TO USE THE 
SOFTWARE.  NO UPDATES, FIXES OR SUPPORTS WILL BE MADE 
AVAILABLE FOR THE SOFTWARE.

7.  NO WARRANTY AND DISCLAIMER OF INDEMNITY
[NO WARRANTY]  THE SOFTWARE IS PROVIDED "AS IS" WITHOUT 
WARRANTY OF ANY KIND, EITHER EXPRESSED OR IMPLIED, 
INCLUDING, BUT NOT LIMITED TO THE IMPLIED WARRANTIES OF 
MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE.  
THE ENTIRE RISK AS TO THE QUALITY AND PERFORMANCE OF THE 
SOFTWARE IS WITH YOU.  SHOULD THE SOFTWARE PROVE 
DEFECTIVE, YOU ASSUME THE ENTIRE COST OF ALL NECESSARY 
SERVICING, REPAIR OR CORRECTION.  SOME STATES OR LEGAL 
JURISDICTIONS DO NOT ALLOW THE EXCLUSION OF IMPLIED 
WARRANTIES, SO THE ABOVE EXCLUSION MAY NOT APPLY TO YOU.  
THIS WARRANTY GIVES YOU SPECIFIC LEGAL RIGHTS AND YOU MAY 
ALSO HAVE OTHER RIGHTS WHICH VARY FROM STATE TO STATE OR 
JURISDICTION TO JURISDICTION.

NEITHER CANON, CANON'S SUBSIDIARIES OR AFFILIATES, THEIR 
DISTRIBUTORS, OR DEALERS NOR CANON'S LICENSORS WARRANT 
THAT THE FUNCTIONS CONTAINED IN THE SOFTWARE WILL MEET 
YOUR REQUIREMENTS OR THAT THE OPERATION OF THE SOFTWARE 
WILL BE UNINTERRUPTED OR ERROR FREE.

[NO LIABILITY FOR DAMAGES]  IN NO EVENT SHALL EITHER CANON, 
CANON'S SUBSIDIARIES OR AFFILIATES, THEIR DISTRIBUTORS 
DEALERS OR CANON'S LICENSORS BE LIABLE FOR ANY DAMAGES 
WHATSOEVER (INCLUDING WITHOUT LIMITATION, LOSS OF BUSINESS 
PROFITS, LOSS OF BUSINESS INFORMATION, LOSS OF BUSINESS 
INTERRUPTION OR OTHER COMPENSATORY, INCIDENTAL OR 
CONSEQUENTIAL DAMAGES) ARISING OUT OF THE SOFTWARE, USE 
THEREOF OR INABILITY TO USE THE SOFTWARE EVEN IF EITHER 
CANON, CANON'S SUBSIDIARIES OR AFFILIATES, THEIR 
DISTRIBUTORS, DEALERS OR CANON'S LICENSORS HAVE BEEN 
ADVISED OF THE POSSIBILITY OF SUCH DAMAGES.  SOME STATES OR 
LEGAL JURISDICTIONS DO NOT ALLOW THE LIMITATION OR 
EXCLUSION OF LIABILITY FOR INCIDENTAL OR CONSEQUENTIAL 
DAMAGES, OR PERSONAL INJURY OR DEATH RESULTING FROM 
NEGLIGENCE ON THE PART OF SELLER, SO THE ABOVE LIMITATION 
OR EXCLUSION MAY NOT APPLY TO YOU.

[RELEASE OF LIABILITY]  TO THE FULL EXTENT PERMITTED BY 
APPLICABLE LAW, YOU HEREBY RELEASE CANON, CANON'S 
SUBSIDIARIES AND AFFILIATES, THEIR DISTRIBUTORS, DEALERS AND 
CANON'S LICENSORS FROM ANY AND ALL LIABILITY ARISING FROM 
OR RELATED TO ALL CLAIMS CONCERNING THE SOFTWARE OR ITS 
USE.

8.  TERM
This Agreement is effective upon your acceptance hereof by the action to 
indicate your acceptance or using the Software and remains in effect until 
terminated.  You may terminate this Agreement by destroying the Software 
including any and all copies thereof.  This Agreement shall also terminate if 
you fail to comply with any terms hereof.  Upon termination of this Agreement, 
in addition to Canon enforcing its respective legal rights, you must then 
promptly destroy the Software including any and all copies thereof.  
Notwithstanding the foregoing, Sections 4, and 7 through 11 shall 
survive any termination of this Agreement.

9.  U.S. GOVERNMENT RESTRICTED RIGHTS NOTICE
The Software is a "commercial item," as that term is defined at 48 C.F.R. 2.101
(October 1995), consisting of "commercial computer software" and "commercial 
computer software documentation," as such terms are used in 48 C.F.R. 12.212 
(September 1995).  Consistent with 48 C.F.R. 12.212 and 48 C.F.R. 227.7202-1 
through 227.7202-4 (June 1995), all U.S. Government End Users shall acquire the
Software with only those rights set forth herein.  Manufacturer is Canon Inc./
30-2, Shimomaruko 3-chome, Ohta-ku, Tokyo 146-8501, Japan.

10.  SEVERABILITY
In the event that any section hereof is declared or found to be illegal by any 
court or tribunal of competent jurisdiction, such section shall be null and 
void with respect to the jurisdiction of that court or tribunal and all the 
remaining provisions hereof shall remain in full force and effect.

11.  ACKNOWLEDGEMENT
BY THE ACTION TO INDICATE YOUR ACCEPTANCE OR USING THE 
SOFTWARE, YOU ACKNOWLEDGE THAT YOU HAVE READ THIS 
AGREEMENT, UNDERSTOOD IT, AND AGREE TO BE BOUND BY ITS TERMS 
AND CONDITIONS.  YOU ALSO AGREE THAT THIS AGREEMENT IS THE 
COMPLETE AND EXCLUSIVE STATEMENT OF AGREEMENT BETWEEN YOU 
AND CANON CONCERNING THE SUBJECT MATTER HEREOF AND 
SUPERSEDES ALL PROPOSALS OR PRIOR AGREEMENTS, VERBAL OR 
WRITTEN, AND ANY OTHER COMMUNICATIONS BETWEEN YOU AND 
CANON RELATING TO THE SUBJECT MATTER HEREOF.  NO AMENDMENT 
TO THIS AGREEMENT SHALL BE EFFECTIVE UNLESS SIGNED BY A DULY 
AUTHORISED REPRESENTATIVE OF CANON.



Should you have any questions concerning this Agreement, or if you desire to 
contact Canon for any reason, please write to Canon's sales subsidiary or 
distributor/dealer, serving the country where you obtained the Products.

***************************************************************************
Copyright CANON INC. 2005

- Canon PostScript(R) 3 emulation Printer Driver - Version 2.77
  for Windows(R) 98/Me/NT4.0/2000/XP/Server 2003
**************************************************************************
This README file contains supplemental information to help you install and
use your PS printer driver software with Microsoft(R) Windows 98, Windows Me,
Windows NT(R) 4.0, Windows 2000, Windows XP and Windows Server(TM) 2003.
As with most software and hardware products, some information is made
available after the development of the manual.  Updated information
regarding this driver software is provided in this README file. If you
require additional assistance, please contact your local Canon company.


Microsoft, Windows and Windows NT are registered trademarks of Microsoft 
Corporation in the United States and/or other countries.
PostScript is trademark of Adobe Systems Incorporated.
PostScript 3 emulation is referred to as PS through this file.

Important
---------
To view the manual in PDF format, Adobe Reader/Adobe Acrobat Reader is 
required. If Adobe Reader/Adobe Acrobat Reader is not installed on 
your system, please download it from the Adobe Systems Incorporated 
website (http://www.adobe.com).


CONTENTS
========
Overview
System Requirements
Installing the Printer Driver 
Installing the PPD File
Accessing the Properties Dialog Box
Accessing Help Information
Cautions, Limitations and Restrictions


Overview
========
This printer driver allows you to print documents from any Windows 98, 
Windows Me, Windows NT 4.0, Windows 2000, Windows XP or Windows Server 2003
application to your printer.

Note
----
* You can change the factory default settings of the printer driver to create 
  customized driver sets using the Canon Driver Configuration Tool. For 
  detailed information about this utility, refer to the Canon Driver 
  Configuration Tool User's Guide .


System Requirements
===================
The Canon PS Printer Driver can be used in the following system environments:

* Operating System Software
  Microsoft Windows 98
  Microsoft Windows Me
  Microsoft Windows NT4.0
  Microsoft Windows 2000
  Microsoft Windows XP
  Microsoft Windows Server 2003

* With Server-Based Computing Environment
  - Compatible Windows Terminal Server (Service)
    Microsoft Windows NT4.0 Terminal Server Edition
    Microsoft Windows 2000 Server
    Microsoft Windows Server 2003
  - Compatible Software
    Citrix MetaFrame XP
    Citrix MetaFrame 1.8
    Citrix MetaFrame Presentation Server 3.0
    Citrix Presentation Server 4.0
  - Compatible Microsoft Cluster Server (MSCS)
    Microsoft Windows 2000 Advanced Server
    Microsoft Windows Server 2003 Enterprise Edition

* Computer 
  Any computer which runs the above operating system software properly. 
  However, at least one of the following output ports is required:

  - parallel printer port (LPT1, LPT2, etc.)
  - USB port 
  - network interface

  The network interface is recommended for the highest quality printing 
  throughput.


Installing the Printer Driver 
============================= 
To use this printer driver with software applications that operate
with Microsoft Windows 98/Me/NT4.0/2000/XP/Server 2003, use the following 
installation procedure.

Note
----
* When using the installer for Winodows NT4.0, Service Pack 6 or later must be 
  installed in your system.
* It is recommended to use the installer for upgrading or adding printer 
  drivers. If you install a new printer driver using the Add Printer Wizard, 
  you must upgrade all existing printer drivers by clicking the New Driver 
  button in the Printer Properties dialog box.
* If you use a SMB (NetBIOS network) printer as a shared printer on the server 
  PC, use the Add Printer Wizard, and select "Network printer"  when installing
  the printer driver.
* Under the Windows NT4.0 Terminal Server environment, you cannot install the 
  printer driver correctly if you execute the installer on the Remote Login 
  screen of the client PC. In this case, install the driver on the Terminal 
  Server. If you want to do so on the Remote Login screen, contact your Canon 
  authorized dealer or Canon authorized service provider.
* If you use the installer under Windows 98/Me, the installation may be 
  suspended depending on the system environment you use. In this case, restart 
  your computer, and then retry the installation.
* If you log on Windows NT4.0/2000/XP/Server 2003 as a Power User and run the 
  installer, the installation may not be completed correctly. In this case, 
  log in as an Administrator, and then retry the installation.
* If you do not restart the computer when a message appears prompting you to do
  so, Microsoft Office may not operate correctly after that. If this happens, 
  restart your computer.
* If the following Canon drivers have been installed for Windows 2000/XP/Server
  2003, it is necessary to restart the computer after the installation.
  - PS v1.00 printer driver
  - PCL5e v4.70 or older printer driver 
  - PCL6 v2.40 or older printer driver
  - Fax v1.40 or older driver
* If you are using Canon PS printer driver V1.00 under Windows NT4.0/2000/XP/
  Server 2003, first update the driver to V1.2x or V1.3x, then install the 
  V2.21 printer driver.
* If you are using the printer auto-creation mechanism in a MetaFrame 
  environment, you may not be able to correctly install this driver 
  using the Installer. If so, restart the MetaFrame Server PC and 
  check the Printers folder (Printers and Faxes folder in Windows XP/
  Server 2003). If any existing printer icons are no longer displayed, 
  re-install the relevant printer drivers in the MetaFrame Server PC 
  using the Add Printer Wizard in the Printers folder. 
  Then, before starting the Installer to install this driver, 
  disconnect all client printers from all the ICA sessions using 
  the ICA Client Printer Configuration utility. After installing 
  the driver, restart the ICA Client Printer Configuration utility 
  and reconnect the printers.
* For Windows Me, updating the driver to version 2.40 or later from versions 
  2.01, 2.10, or 2.20 may cause problems with some paper settings. The paper 
  size or paper type settings for each paper source specified in the Form to 
  Tray Assignment dialog may not update correctly. The Form to Tray Assignment 
  dialog can be opened by clicking the corresponding button in the 
  Configuration sheet. 

To install using the Installer:
1. Insert the Printer Driver Software CD-ROM into the CD-ROM drive.
2. Double-click the My Computer icon, and then double-click the CD-ROM drive 
   icon.
3. Double-click the PS, and uk_eng folder icons, and then double-click the 
   Setup.exe icon to start the installation process.
4. In the first dialog box of the Printer Driver Setup Wizard, click the Next
   button, and then follow the instructions on the screen.
5. Select Manually Set Port to Install, and then click the Next button.
6. If the dialog box to select items to install is displayed, select PS3
   Printer Driver and click the Next button.
7. If the dialog box to select how to execute the setup is displayed, select 
   Add Printers, or Add Printers and Update Drivers, and then click the Next 
   button.
8. Select the driver you want to install from Printer List and click the Add
   button.
9. Check that the driver you want to install is selected in the Printer 
   Driver Setup Wizard dialog box. Then click the Next button.
10.Select a Port from drop-down menu or by clicking the Add Port button.
   Then click the Next button.
11.In the next dialog box, check the installation settings, and then click the
   Start button.
12.After the files are copied, click the Exit button to finish the 
   installation program.

You are now ready to print from any Windows software application.

Note:
* You can add a new driver without affecting existing driver if you select Add 
  Printers for step 8. If you select Add Printers and Update Drivers, all 
  existing drivers are updated automatically when you add a new driver.
* If you are using a shared printer in the Print Server (Point and Print)
  environment, it is necessary to install Canon Driver Information Assist
  Service in the server PC in order to set up the printer configuration
  automatically or to use the Job Accounting feature.
* If you are using an operating system equipped with Windows Firewall, a 
  message which asks if you want to change the Windows Firewall setting is 
  displayed during the installation.
  - If you select Yes, Windows Firewall will be configured to unblock the 
    connection for Canon Driver Information Assist Service, so that you can 
    set up the printer configuration automatically or use the Job Accounting
    feature.
  - If you select No, you cannot use Canon Driver Information Assist Service.

To install using the Add Printer Wizard:
1. Click the Start button, point to Settings, and then click Printers.
2. In the Printers folder, double-click the Add Printer icon to start the Add 
   Printer Wizard.
3. Confirm the Wizard is started, and then click the Next button.
4. Follow the instructions on the screen to continue with the installation.
5. Insert the Printer Driver Software CD-ROM into the CD-ROM drive, and then 
   click the Have Disk button.
6. Click the Browse button to select the folder of the driver you want to 
   install, and then click the OK button. 
   - Windows 98/Me: \PS\uk_eng\win98_me
   - Windows NT4.0: \PS\uk_eng\winnt40
   - Windows 2000/XP/Server 2003: \PS\uk_eng\win2k_xp

7. Select your printer model from Printers, and then click the Next button.  
8. Follow the instructions on the screen to continue, and then click the 
   Finish button to start copying the files.

You are now ready to print from any Windows software application.

To install using a USB connection (Windows 98/Me/2000/XP/Server 2003):
For iR C2570, 2570C, C2620, C3200, C3220, C3100, 3100C, C3170, 3170C, C5800, 
5800C, C5870, 5870C, C6800, 6800C, C6870, 6870C, 105PLUS, 2230, 2830, 
2270/2870, 3530, 3570/4570, 5570/6570, 8070, 85PLUS, and 9070, you can print 
in a USB environment. Install the printer driver through a USB connection.

1. Insert the Printer Driver Software CD-ROM into the CD-ROM drive.
2. Double-click the My Computer icon, and then double-click the CD-ROM drive 
   icon.
3. Double-click the PS, and uk_eng folder icons, and then double-click the 
   Setup.exe icon to start the installation process.
4. In the first dialog box of the Printer Driver Setup Wizard, click the Next
   button, and then follow the instructions on the screen.
5. Select Install with USB Connection, and then click the Next button.
6. Click the Yes button in the message box asking if you want to start the 
   installation.
7. When a dialog box prompts, connect the USB plug, and then turn the printer
   on.
8. After the files are copied, click the Finish button to finish the 
   installation program.


Installing the PPD File
========================
The PPD file for PageMaker V6.52 or later and QuarkXPress 4.x provided in the 
CD-ROM is not be installed in the appropriate folder with the usual 
installation process. In order to use the iR series features in the 
Print dialog box or Page Setup dialog box of these applications, follow the 
procedure below to copy the PPD file into the appropriate folder.
For applications other than the above, use the PPD file for PageMaker 6.52 or
later.

To copy the PPD file:
1. Insert the CD-ROM into the CD-ROM drive and select the My Computer icon 
   on the Desktop.
2. Select the CD-ROM drive icon and select the following folder.
   PageMaker 6.52 or later: PS_PPD\uk_eng\your printer name\pm
   QuarkXPress 4.x: PS_PPD\uk_eng\your printer name\qx
3.Copy the PPD file (Cnir50e1.ppd) in the above folder into the following 
   folder.
   PageMaker 6.52: \PM65\RSRC\usenglish\PPD4 (*1)
   PageMaker 7.00: \PageMaker 7.0\RSRC\usenglish\PPD4 (*1)
   QuarkXPress 4.x: \Windows\system (*2)

   (*1) The user can change the folder name "PM65" or "PageMaker 7.0" when 
        installing the application.
   (*2) The user can specify the folder where to copy the PPD file by using 
        PPD Manager. The default folder is \Windows\system.


Accessing the Properties Dialog Box
======================================
The Properties dialog box contains several sheets that allow you to
setup and control your printer.  To access the Properties dialog box, use one 
of the following procedures, depending on your version of Windows:

Procedure for Windows 98/Me
---------------------------
To access from the Desktop:
1. Click the Start button, point to Settings, and then click Printers.
2. Right-click the printer icon for your printer in the Printers folder, and 
   then click Properties.

To access from within an application:
1. Click the Print command to display the Print dialog box.
2. Select your printer name from the drop-down list box, and then click the 
   Properties button.

Procedure for Windows NT4.0/2000/XP/Server 2003
-----------------------------------------------
To access from the Desktop:
1. Click the Start button, point to Settings, and then click Printers.
2. Right-click the printer icon for your printer in the Printers folder, and 
   then click Properties to open the Printer Properties dialog box, or click 
   Document Defaults (Windows NT4.0) or Printing Preferences (Windows 2000/XP/
   Server 2003) to open the Document Properties dialog box.

To access from within an application:
1. Click the Print command to display the Print dialog box.
2. Select your printer name from the drop-down list box, and then click the 
   Properties button.


Accessing Help Information
==========================
From the Properties dialog box, you can click the Help button to
display the information about the PS printer driver. You can also 
click the ? button in the upper right corner of dialog boxes and then click a
specific item in a dialog box for help with that item.


Cautions, Limitations and Restrictions
======================================
1. For Windows NT4.0, when using the Watermark function and printing from
   CorelDRAW, Illustrator or Acrobat, more time is required to release the 
   application and complete the print job.

2. When printing Euro symbols, select Symbol if using printer fonts, or use 
   TrueType fonts. True Type fonts can be selected by doing any of the 
   following operation:
    - Click the Details button in the Quality Sheet, and select Always
      Send TrueType Fonts in the Detailed Settings dialog box.
    - Click the Font Settings button in the Configuration sheet (Windows
      98/Me) or Device Settings sheet (Windows NT4.0/2000/XP/Server 2003),
      and select Download for the TrueType fonts you want to use in the
      Font Substitution Table.

3. When using the collate function of the application and Saddle Stitch is
   specified for Booklet Printing, all paper will be sorted and saddle 
   stitched.
   When using Saddle Stitch function for Booklet Printing, disable the collate
   function of the application.

4. To speed up printing when the printer is connected via a network, Binary is
   recommended as the Data Protocol in the PS Options dialog box which is 
   displayed from the Configuration sheet (Windows 98/Me) or Device 
   Settings sheet (Windows NT4.0/2000/XP/Server 2003).

5. When Overlay Printing, use the overlay form whose size, orientation and Page
   Layout is the same as those of the document you are going to print.

6. When creating a custom paper size in the Print Server Properties dialog box 
   of Windows NT 4.0/2000/XP/Server 2003, specify the margins as follows:
   - iR105/8500: 0.45cm/0.18in or more
   - iR C2620/C3200/C3220: 0.25cm/0.10in or more
   - Other printers: 0.40cm/0.16in or more

7. When creating a overlay form file in one machine operating Windows 
   NT4.0/2000/XP/Server 2003, you cannot specify another machine operating 
   Windows NT4.0/2000/XP/Server 2003 in the network as the place to save the 
   new form file. 

8. Specify a NetWare Server name or NDS tree name up to 15 characters.

9. For Windows 2000/XP/Server 2003 when installing with Add Printer from the 
   Printer Folder, the Cannot find Digital Signature message may appear.
   If this message appears, continue with the installation.  The printer will
   install correctly.

10.When you store a landscape document in the Mail Box of the printer, the 
   staple position displayed on the printer control panel differs from the 
   setting of the printer driver. Also, if you specify the staple position of 
   a landscape document stored in the Mail Box from the printer control panel, 
   the actual staple position of the output document may not correspond with 
   the orientation specified.

11.If you select Print to file setting in the Print dialog box when printing a 
   document from Microsoft Word 2002, specify On for PS Output from Application
   in the Configuration sheet (Windows 98/Me) or Device Settings sheet 
   (Windows 2000/XP/Server 2003) prior to printing.

12.When you select Paper Type for Select by in the Paper Source sheet, select 
   Same Paper for All Pages for Paper Selection if you want to use Tab Paper to
   print a document. If you specify several different paper types to print each
   pages of a document, the print out on the Tab Paper may not be correct.

13.When printing from Microsoft Word 2002 or Lotus 1-2-3 under Windows NT4.0, 
   Watermark settings in the Properties dialog box that is displayed by right-
   clicking the Properties button in the Print dialog box may not work 
   correctly. In this case, specify the Watermark settings in advance in the 
   Printer Properties dialog box that can be accessed from the Printers folder 
   in the Control Panel. 

14.When you select Auto or On for PS Output from Application in the 
   Configuration sheet (Windows 98/Me) or Device Settings sheet (Windows 
   2000/XP/Server 2003), the print out from Illustrator may not be correct.
   In this case, open the Font Settings dialog box from the Configuration sheet
   (Windows 98/Me) or Device Settings sheet (Windows 2000/XP/Server 2003),
   and then download the printer font you want to use, or open the Detailed 
   Settings dialog box from the Quality sheet, and then select Always Send 
   TrueType Fonts for Substitution.

15. When printing from QuarkXPress, the document may not be printed and blank 
    pages are output. In this case, select On for PS Output from Application 
    in the Configuration sheet (Windows 98/Me) or Device Settings sheet 
    (Windows 2000/XP/Server 2003).

16. Some applications send the PostScript command to the printer directly when 
    using the PostScript printer driver. For these applications, the following 
    functions may not be available.
    - From the Page Setup sheet: Page Layout, Watermark, Manual Scaling
    - From the Paper Source sheet: Paper Selection
    - From the Quality sheet : Print as Negative Image, Print as Mirror Image

    * For Windows 98/Me/2000/XP/Server 2003, you can use the above 
      functions when the PS Output from Application setting in the 
      Configuration or Device Settings sheet is set to Off.

17. The printed output may not be correct when printing from applications 
    that use the ROP command, which is not supported by PostScript language. 
    For example, the printed results of grayscale printing for Micrografx 
    Designer or Word Art for Microsoft Word are incorrect.
    For Windows 98/Me/2000/XP/Server 2003, selecting On for PS Output from
    Application in the Configuration or Device Settings sheet may solve the 
    problem. 

18. When printing a document to which EPS objects are attached, the printed 
    output may not be correct. 
    For Windows 98/Me/2000/XP/Server 2003, selecting On for PS Output
    from Application in the Configuration or Device Settings sheet may solve 
    the problem. 

19. For Window XP/Server 2003, it is necessary to use TCP/IP as a network 
    protocol in order to set up the printer configuration automatically when 
    using a Remote Desktop environment, or when Windows is shared by multiple 
    users.

20. When inserting inserted sheets into the document, if you accidentally 
    specify a drawer that contains tab paper as the paper source for the 
    inserted sheets, the paper source automatically returns to the plain paper 
    setting.

21. If you select Rotate Print Data 180 Degrees in the Advanced Settings dialog
    box when any Finishing option is selected, the document may output in an 
    unexpected style.

22. For iR105, 105PLUS, 7200, 8070, 8500, 85PLUS, and 9070 under Windows 
    98/Me/2000/XP/Server 2003, when using booklet printing with saddle stitch, 
    the printed cover page loaded from Document Insertion Unit may be attached 
    upside down. If this occurs, put the cover page in the Document Insertion 
    Unit in the opposite direction.

23. For Windows 2000/XP/Server 2003, when printing a document with a banner 
    page attached from the server PC under the NetWare environment, two copies 
    of the banner page may be output. 

24. According to the version of the PS printer driver, the available options 
    for Halftones in the Quality sheet differ as below.
    - V2.1x: [Standard] is supported, [Pattern 7] is not supported
    - V2.20 and later: [Standard] is not supported, [Pattern 7] is supported
    For Windows 98/Me under environments where the PS printer driver v2.1x for
    iR C3200 is installed, [Standard] will be not available and [Pattern 7] 
    will be available for the iR C3200 driver after you install the PS printer
    driver of v2.20 or later for iR C2620, C3100, 3100C, C3220, C5800, 5800C, 
    C6800, or 6800C.

25. When printing from IllustratorCS, a message is displayed that shows the PPD
    file you specified is invalid. However, clicking OK in the message box 
    continues printing.

<END OF README.TXT>
